LX_VM-TV_Driver Readme

--------------------------------------------------------
!!! WARNING !!!
READ DAUGHTERCARD USER'S GUIDE FOR CRITICAL INSTALL PROCEDURES OR YOUR BOARD WILL LOSE ALL VIDEO FUCTIONS!!!
--------------------------------------------------------

This driver is a customization of the standard AMD Geode LX video driver.  It is designed to support the Geode VM-TV TV-out daughter card.  The VM-TV daughtercard contains a Focus Enhancements FS455 encoder supporting the following modes:

SDTV:
Source resolutions of 640x480, 800x600 & 1024x768
Output NTSC & PAL via Composite (CVBS) and S-Video

HDTV:
525p, 720p & 1080i

Notes:
Due to limitations in Windows XP, NTSC modes, PAL modes and SCART mode are compiled in separate driver packages.

--------------------------------------------------------

NTSC Modes Driver:  lx_fs454_ntsc.inf
Contains modes for
SDTV, Composite & S-Video at 640x480, 800x600, 1024x768
HDTV, Component at 525p, 720p, 1080i

PAL Modes Driver:   lx_fs454_ntsc.inf
Contains modes for
SDTV, Composite & S-Video at 640x480, 800x600, 1024x768
HDTV, Component at 525p, 720p, 1080i

SCART Mode Driver:
Not Complete
