     VIA Chipset AGP Driver Component for Windows XP Embedded SP1
                               1/7/2005
            Copyright (C) 2002-2005 VIA Technologies, INC.

1. Release note
   This package is ver 1.0, adapted from logo'ed package VIA_AGP_V443EP3.zip.
   Users are advised to contact VIA for information about the usage
   of the component for their specific embedded platforms.

   VIA provides the user with this sample component implementation,
   to ease development and test effort. The user, however,
   is advised to obtain the latest available driver and author
   his or her own components.

2. File description
   This package contains 5 files as described below.

                                       Readme.txt       this file
01/06/2005  05:24 PM          167,426 VIAAGP1_v10.sld  driver component
07/30/2003  12:45 AM             8,850 viaagp1.cat
07/02/2003  04:42 AM           27,904 viaagp1.sys
07/02/2003  04:42 AM             4,187 VIAAGP1.INF


3. Import the driver component
(1) Copy all the files to a directory, e.g. "D:\VIADRIVERS\AGP443ep3\".
(2) Create a directory, e.g. "D:\VIA_Repositories\", if there is
    none.
(3) Open Component Database Manager under Microsoft Windows
    Embedded Studio.
(4) Click on the "Repository" and then "Repository Roots..." buttons.
    Type in the complete path of the repositories directory,
    for example "D:\VIA_Repositories\". Click on the "Add" button
    and answer "Yes".
(5) Click on the "Database", "Import...", and then "..." buttons.
    Navigate to directory "D:\VIADRIVERS\AGP443ep3\" and then choose
    the .SLD file. Next, pull down "Repository root" drop-down
    and select "D:\VIA_Repositories\". Click on the "Import" and
    then "Close" buttons to close the dialog.
(6) Close the "Component Database Manager".
