binary_file lx_CRT_2_modes.out
inf_file lx_CRT_2_modes.inf
disk_id "CRT 2 modes driver"
manual_display_mode_count 2

manual_mode_0 bpp_mask 0x6
manual_mode_0 output_path 0
manual_mode_0 output_space DF_OUTPUT_RGB
manual_mode_0 flicker_strength 0
manual_mode_0 line_double_video_on_interlaced 0
manual_mode_0 border_color 0
manual_mode_0 premode_smbus_count 0
manual_mode_0 postmode_smbus_count 11
manual_mode_0 custom_coefficients 0
manual_mode_0 configure_vop 0

manual_mode_0\manual_timings flags VG_MODEFLAG_HIGH_BAND
manual_mode_0\manual_timings src_width 1920
manual_mode_0\manual_timings src_height 1440
manual_mode_0\manual_timings mode_width 0
manual_mode_0\manual_timings mode_height 0
manual_mode_0\manual_timings panel_width 0
manual_mode_0\manual_timings panel_height 0
manual_mode_0\manual_timings panel_tim1 0
manual_mode_0\manual_timings panel_tim2 0
manual_mode_0\manual_timings panel_dither_ctl 0
manual_mode_0\manual_timings panel_pad_sel_low 0
manual_mode_0\manual_timings panel_pad_sel_high 0
manual_mode_0\manual_timings hactive 0x0780
manual_mode_0\manual_timings hblankstart 0x780
manual_mode_0\manual_timings hsyncstart 0x818
manual_mode_0\manual_timings hsyncend 0x8F0
manual_mode_0\manual_timings hblankend 0x0A60
manual_mode_0\manual_timings htotal 0x0A60
manual_mode_0\manual_timings vactive 0x05A0
manual_mode_0\manual_timings vblankstart 0x05A0
manual_mode_0\manual_timings vsyncstart 0x05A1
manual_mode_0\manual_timings vsyncend 0x05A4
manual_mode_0\manual_timings vblankend 0x05E8
manual_mode_0\manual_timings vtotal 0x05E8
manual_mode_0\manual_timings vactive_even 0
manual_mode_0\manual_timings vblankstart_even 0
manual_mode_0\manual_timings vsyncstart_even 0
manual_mode_0\manual_timings vsyncend_even 0
manual_mode_0\manual_timings vblankend_even 0
manual_mode_0\manual_timings vtotal_even 0
manual_mode_0\manual_timings frequency 0x1550000

manual_mode_0\postmode_smbus base_0                 0x42
manual_mode_0\postmode_smbus addr_0                 0x00
manual_mode_0\postmode_smbus data_0                 0x05
manual_mode_0\postmode_smbus base_1                 0x42
manual_mode_0\postmode_smbus addr_1                 0x0E
manual_mode_0\postmode_smbus data_1                 0x06
manual_mode_0\postmode_smbus base_2                 0x42
manual_mode_0\postmode_smbus addr_2                 0x10
manual_mode_0\postmode_smbus data_2                 0x3A
manual_mode_0\postmode_smbus base_3                 0x42
manual_mode_0\postmode_smbus addr_3                 0x80
manual_mode_0\postmode_smbus data_3                 0x3B
manual_mode_0\postmode_smbus base_4                 0x42
manual_mode_0\postmode_smbus addr_4                 0x53
manual_mode_0\postmode_smbus data_4                 0x3C
manual_mode_0\postmode_smbus base_5                 0x42
manual_mode_0\postmode_smbus addr_5                 0x80
manual_mode_0\postmode_smbus data_5                 0x6A
manual_mode_0\postmode_smbus base_6                 0x42
manual_mode_0\postmode_smbus addr_6                 0xC3
manual_mode_0\postmode_smbus data_6                 0x6B
manual_mode_0\postmode_smbus base_7                 0x42
manual_mode_0\postmode_smbus addr_7                 0x06
manual_mode_0\postmode_smbus data_7                 0x7B
manual_mode_0\postmode_smbus base_8                 0x42
manual_mode_0\postmode_smbus addr_8                 0x18
manual_mode_0\postmode_smbus data_8                 0x85
manual_mode_0\postmode_smbus base_9                 0x42
manual_mode_0\postmode_smbus addr_9                 0x06
manual_mode_0\postmode_smbus data_9                 0x86
manual_mode_0\postmode_smbus base_10                0x42
manual_mode_0\postmode_smbus addr_10                0x0C
manual_mode_0\postmode_smbus data_10                0xC9

manual_mode_1 bpp_mask 0x6
manual_mode_1 output_path 0
manual_mode_1 output_space DF_OUTPUT_RGB
manual_mode_1 flicker_strength 0
manual_mode_1 line_double_video_on_interlaced 0
manual_mode_1 border_color 0
manual_mode_1 premode_smbus_count 0
manual_mode_1 postmode_smbus_count 11
manual_mode_1 custom_coefficients 0
manual_mode_1 configure_vop 0

manual_mode_1\manual_timings flags VG_MODEFLAG_LOW_BAND
manual_mode_1\manual_timings src_width 800
manual_mode_1\manual_timings src_height 600
manual_mode_1\manual_timings mode_width 0
manual_mode_1\manual_timings mode_height 0
manual_mode_1\manual_timings panel_width 0
manual_mode_1\manual_timings panel_height 0
manual_mode_1\manual_timings panel_tim1 0
manual_mode_1\manual_timings panel_tim2 0
manual_mode_1\manual_timings panel_dither_ctl 0
manual_mode_1\manual_timings panel_pad_sel_low 0
manual_mode_1\manual_timings panel_pad_sel_high 0
manual_mode_1\manual_timings hactive 0x0320
manual_mode_1\manual_timings hblankstart 0x0320
manual_mode_1\manual_timings hsyncstart 0x0348
manual_mode_1\manual_timings hsyncend 0x0398
manual_mode_1\manual_timings hblankend 0x0410
manual_mode_1\manual_timings htotal 0x0410
manual_mode_1\manual_timings vactive 0x0258
manual_mode_1\manual_timings vblankstart 0x0258
manual_mode_1\manual_timings vsyncstart 0x025C
manual_mode_1\manual_timings vsyncend 0x025F
manual_mode_1\manual_timings vblankend 0x0274
manual_mode_1\manual_timings vtotal 0x0274
manual_mode_1\manual_timings vactive_even 0
manual_mode_1\manual_timings vblankstart_even 0
manual_mode_1\manual_timings vsyncstart_even 0
manual_mode_1\manual_timings vsyncend_even 0
manual_mode_1\manual_timings vblankend_even 0
manual_mode_1\manual_timings vtotal_even 0
manual_mode_1\manual_timings frequency 0x2D0000

manual_mode_1\postmode_smbus base_0                 0x42
manual_mode_1\postmode_smbus addr_0                 0x00
manual_mode_1\postmode_smbus data_0                 0x05
manual_mode_1\postmode_smbus base_1                 0x42
manual_mode_1\postmode_smbus addr_1                 0x0E
manual_mode_1\postmode_smbus data_1                 0x06
manual_mode_1\postmode_smbus base_2                 0x42
manual_mode_1\postmode_smbus addr_2                 0x10
manual_mode_1\postmode_smbus data_2                 0x3A
manual_mode_1\postmode_smbus base_3                 0x42
manual_mode_1\postmode_smbus addr_3                 0x80
manual_mode_1\postmode_smbus data_3                 0x3B
manual_mode_1\postmode_smbus base_4                 0x42
manual_mode_1\postmode_smbus addr_4                 0x53
manual_mode_1\postmode_smbus data_4                 0x3C
manual_mode_1\postmode_smbus base_5                 0x42
manual_mode_1\postmode_smbus addr_5                 0x80
manual_mode_1\postmode_smbus data_5                 0x6A
manual_mode_1\postmode_smbus base_6                 0x42
manual_mode_1\postmode_smbus addr_6                 0xC3
manual_mode_1\postmode_smbus data_6                 0x6B
manual_mode_1\postmode_smbus base_7                 0x42
manual_mode_1\postmode_smbus addr_7                 0x06
manual_mode_1\postmode_smbus data_7                 0x7B
manual_mode_1\postmode_smbus base_8                 0x42
manual_mode_1\postmode_smbus addr_8                 0x18
manual_mode_1\postmode_smbus data_8                 0x85
manual_mode_1\postmode_smbus base_9                 0x42
manual_mode_1\postmode_smbus addr_9                 0x06
manual_mode_1\postmode_smbus data_9                 0x86
manual_mode_1\postmode_smbus base_10                0x42
manual_mode_1\postmode_smbus addr_10                0x0C
manual_mode_1\postmode_smbus data_10                0xC9